Expert Tank Cleaning in Guduvancheri, OMR & Chennai

Chat Now 90423 65444
#1 in Chennai

# Mechanised Sump & Tank Cleaning

Don't bathe in bacteria. We use a 6-stage German technology to remove 100% sludge, algae, and viruses from your underground sumps and overhead tanks.

Sludge Removal High Pressure Clean UV Sterilization
+500

Trusted by 1000+ Homes in Chennai

FAST RESPONSE

### Get a Free Quote

Fill the form to get pricing in 5 mins.

Your Name
Tank Type
Capacity (Litres)
Mobile Number

## Is Your Water Sump Breeding Disease?

In Chennai's humid climate, underground sumps become a breeding ground for bacteria, algae, and bloodworms. Sediment from metro water settles at the bottom, creating a layer of sludge that manual cleaning cannot fully remove.

Risks of Dirty Tanks:

- Skin allergies & Hair fall
- Waterborne diseases (Typhoid/Cholera)
- Clogged tap filters and low pressure

Speak to a Hygiene Expert

100% Sludge Removal

Vacuum Technology

Our Technology

## 6-Stage Mechanised Cleaning Process

We don't just send a labourer to scrub. We send a team with industrial equipment.

1

### Mechanized Dewatering

High-speed industrial pumps to empty your tank completely.

2

### Sludge Removal

Suctioning out thick bottom sludge and disposal.

3

### High Pressure Scrubbing

Industrial jets blast away algae and calcification from walls.

4

### Vacuum Cleaning

Wet vacuum removes remaining dirty water and fine dust.

5

### Anti-Bacterial Spray

Food-grade organic spray to sanitise the surface.

6

### UV Radiation Treatment

Final sterilization using UV light to kill bacteria. (Premium)

## Transparent Pricing

Tank Capacity | Overhead Tank (Plastic) | Underground Sump (Concrete)
--- | --- | ---
Up to 1,000 Litres | ₹ 999 | ₹ 1,699
1,001 - 5,000 Litres | ₹ 1,499 | ₹ 0.40 / Litre
5,001 - 10,000 Litres | ₹ 0.25 / Litre | ₹ 0.35 / Litre
Above 10,000 Litres | Call for Custom Quote

*Prices are indicative. Final quote depends on tank condition.

Book Service Now

## Tank Cleaning FAQs

How long does the cleaning process take?

For a standard 5000L sump and 1000L overhead tank, the process typically takes 2-4 hours depending on the amount of sludge.

Is the UV treatment safe for drinking water?

Yes, UV radiation is a physical disinfection method that leaves no chemical residue, making it perfectly safe for drinking water tanks.

How much water do we need to save before you come?

We recommend using up most of the water before our arrival to avoid wastage. We will dewater the remaining 10-20% which usually contains the sediment.

### What Our Customers Say

Chat
CALL NOW